<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;b&gt;HAPCAN UNIV 3 library&lt;/b&gt;</description>
<packages>
<package name="UNIV3CPU">
<description>HAPCAN &lt;b&gt;UNIV 3 CPU&lt;/b&gt; processor
(http://hapcan.com)</description>
</package>
<package name="EM500">
<description>Tibbo EM500 programable ethernet module</description>
</package>
<package name="SOT-223">
<description>SOT-223</description>
</package>
<package name="SO-08">
<description>150-mil body, package type SN</description>
</package>
<package name="SOT-23-6">
<description>SOT-23-6</description>
</package>
<package name="SOT-23">
<description>SOT-23</description>
</package>
<package name="SO-20W">
<description>20-Lead (300mil Wide Body) Small Outline Package</description>
</package>
<package name="TO-252">
<description>TO-252</description>
</package>
<package name="DO-214">
<description>HAPCAN DO-214AA</description>
</package>
<package name="0805">
<description>0805 package</description>
</package>
<package name="SIP-5">
<description>Header SIP-5</description>
</package>
<package name="TO220H">
<description>HAPCAN TO-220 horizontal 3pin</description>
</package>
<package name="TO220V">
<description>HAPCAN TO-220 vertical 3 pin</description>
</package>
<package name="TO-92">
<description>TO-92</description>
</package>
<package name="CRYSTAL-HC49V">
<description>CRYSTAL</description>
</package>
<package name="SO-16">
<description>16-pin 150-mil body</description>
</package>
<package name="1210">
<description>1210 capacior package</description>
</package>
<package name="SMC_B">
<description>SMB capacior package</description>
</package>
<package name="SMC_C">
<description>SMC capacior package</description>
</package>
<package name="SMC_D">
<description>SMD capacior package</description>
</package>
<package name="SIP-1">
<description>HEADER SIP 1</description>
</package>
<package name="ARK2-5X9MM">
<description>ARK2 - 9mm  thick</description>
</package>
<package name="ARK3-5X9MM">
<description>ARK3 - 9mm thick</description>
</package>
<package name="DIL-24">
<description>HAPCAN Header DIL-24</description>
</package>
<package name="RELAY_PE">
<description>PCB Relay, type PE (SHRACK), bistable/monostable version 5 A</description>
</package>
<package name="RELAY_PE+RT">
<description>Relay RT and PE on the same pcb</description>
</package>
<package name="VARISTOR1">
<description>VARISTOR version 1</description>
</package>
<package name="HEADER-2X8">
<description>HAPCAN 2x8pin connector</description>
</package>
<package name="DO-214_TRANSIL2">
<description>DO-214AA bidirectional transil</description>
</package>
<package name="ARK2-5X10,5MM">
<description>ARK2 - 10.5mm  thick</description>
</package>
<package name="ARK3-5X10.5MM">
<description>ARK2 - 10.5mm  thick</description>
</package>
<package name="RJ45-PCB-SOCKET">
<description>RJ45 pcb socket</description>
</package>
<package name="ARK2-7.5X10.5MM">
<description>ARK2 - raster 7.5mm, 10.5mm  thick</description>
</package>
<package name="ARK3-7.5X10.5MM">
<description>ARK3 - raster 7.5mm, 10.5mm  thick</description>
</package>
<package name="CAP-5X10.5">
<description>Electrolytic capacitor, raster 5, diameter 10.5mm, drill 1mm</description>
</package>
<package name="SIP-2">
<description>Header SIP-2</description>
</package>
<package name="CHOKE-DL16">
<description>Choke DL16</description>
</package>
<package name="CRYSTAL-TC26V">
<description>Crystal  TC26V</description>
</package>
<package name="CAP-5X14">
<description>Electrolytic capacitor, raster 5, diameter 14mm, drill 1.5mm</description>
</package>
<package name="RJ45-PCB-SOCKET+TRAFO">
<description>RJ45 pcb socket with trafo and LEDs</description>
</package>
<package name="HEADER-2X8-MIRRORED">
<description>HAPCAN 2x8pin connector mirrored</description>
</package>
<package name="SUB-D9FH-7.2MM">
<description>HAPCAN SUB-D 9 pin female horizontal connector</description>
</package>
<package name="TO220V-2">
<description>HAPCAN TO-220 vertical 2 pin</description>
</package>
<package name="DIL-08">
<description>HAPCAN DIL-08</description>
</package>
<package name="SOD-80">
<description>HAPCAN SOD-80 (MINIMELF)</description>
</package>
<package name="CAP-2X5">
<description>Electrolytic capacitor, raster 2mm, diameter 5mm, drill 0.7mm</description>
</package>
<package name="CRYSTAL-TC38H">
<description>Crystal TC38H</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="CHOKE-10X25">
<description>Choke 10mm x 25mm dia</description>
</package>
<package name="CAP-15X5">
<description>Capacitor, raster 15mm, wide 5mm, drill 1mm</description>
</package>
<package name="RES-15X5">
<description>Resistor, raster 15mm, diameter 5mm, drill 1mm</description>
</package>
<package name="1206_LED-R">
<description>1206 LED for reversed mounting</description>
</package>
<package name="HEADER-2X8_SMD">
<description>HAPCAN 16pin smd connector</description>
</package>
<package name="TO-92_SMD">
<description>HAPCAN TO-92 smd</description>
</package>
<package name="TOUCH_SENSOR">
<description>Touch sensor pad</description>
</package>
<package name="DIL-08W">
<description>HAPCAN DIL-08 wide (8mm clearance)</description>
</package>
<package name="TO262-V">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="TO262-H">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="TO247V">
<description>HAPCAN TO-247 vertical, 3 pin, grid 5.6 mm</description>
</package>
<package name="TO247H">
<description>HAPCAN TO-247 horizontal, 3 pin, grid 5.6 mm</description>
</package>
<package name="RECTIFIER_KBL">
<description>DIOTEC RECTIFIER KBL grid 5mm</description>
</package>
<package name="RECTIFIER_KBP">
<description>DC COMPONENTS RECTIFIER KBP grid 3.81 mm</description>
</package>
<package name="FUSE-LITTLEFUSE">
<description>LITTLEFUSE fuse</description>
</package>
<package name="FUSE-HOLDER-V">
<description>Vertical fuse holder</description>
</package>
<package name="SO-16W">
<description>16-Lead (300mil Wide Body) Small Outline Package</description>
</package>
<package name="SMD4">
<description>&lt;b&gt;SMD 4&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/83673/sfh618.pdf</description>
</package>
<package name="DO-213">
<description>HAPCAN DO-213AB</description>
</package>
<package name="DIL-04W">
<description>HAPCAN DIL-04 wide (8mm clearance)</description>
</package>
<package name="2512">
<description>2512 package</description>
</package>
<package name="RECTIFIER_DBS">
<description>DC COMPONENTS RECTIFIER DBS</description>
</package>
<package name="CAP-10X6">
<description>Capacitor, raster 10mm, wide 6mm, drill 0.8mm</description>
</package>
<package name="TO-269AA">
<description>TO-269AA</description>
</package>
<package name="2010">
<description>2010 package</description>
</package>
<package name="HEADER-2X4">
<description>HAPCAN 2x4pin connector</description>
</package>
<package name="HEADER-2X4-MIRRORED">
<description>HAPCAN 2x4pin connector mirrored</description>
</package>
<package name="RELAY_RT_SPST">
<description>PCB Relay, type RT (SCHRACK), bistable/monostable version 16 A - SPST (single pole, single throw)</description>
</package>
<package name="RELAY_RT">
<description>PCB Relay, type RT (SHRACK), bistable/monostable version 16 A</description>
</package>
<package name="VARISTOR2">
<description>VARISTOR raster 5mm</description>
</package>
<package name="HEADER-1X1.3">
<description>Header 1x 1.3mm diameter</description>
</package>
<package name="RELAY_SNR_SPDT_V">
<description>Slim PCB Relay, type SNR (SCHRACK), monostable version 6 A - SPDT (single pole, double throw) - vertical</description>
</package>
<package name="RELAY_SNR_SPDT_H">
<description>Slim PCB Relay, type SNR (SCHRACK), monostable version 6 A - SPDT (single pole, double throw) - horizontal</description>
</package>
<package name="VARISTOR3">
<description>VARISTOR raster 7.5mm</description>
</package>
<package name="SIP-5A">
<description>Header SIP-5A</description>
</package>
<package name="1206">
<description>1206 package</description>
</package>
<package name="CHOKE-DER0705">
<description>Choke DER0705</description>
</package>
<package name="HEATSINK_HS-003">
<description>HEATSINK STONECOLD HS-003</description>
</package>
<package name="RES-3.8X3V">
<description>Resistor, raster 3.8mm, diameter 3mm, drill 0.8mm, vertical</description>
</package>
<package name="FUSE-UMT">
</package>
<package name="FUSE-7.5">
</package>
<package name="HEATSINK_HS-123">
<description>HEATSINK STONECOLD HS-123</description>
</package>
<package name="TO220V-3">
<description>HAPCAN TO-220 vertical 3 pin</description>
</package>
<package name="SOT-23-5">
<description>SOT-23-5</description>
</package>
<package name="SO-28W">
<description>28-Lead (300mil Wide Body) Small Outline Package</description>
</package>
<package name="MKKDS1/8-3,5">
<description>Terminal block MKKDS 1/8-3,5</description>
</package>
<package name="VARISTOR4">
<description>VARISTOR raster 10mm</description>
</package>
</packages>
<symbols>
<symbol name="UNIV3CPU">
<pin name="!MCLR!/RE3"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="VDDCORE"/>
<pin name="RA5/AN4"/>
<pin name="VSS@1"/>
<pin name="OSC1/CLKIN/RA7"/>
<pin name="OSC2/CLKOUT/RA6"/>
<pin name="RC0/SCLKI"/>
<pin name="RC1/ISOSCI"/>
<pin name="RC2/CCP2"/>
<pin name="RC3/SCL/SCK"/>
<pin name="RC4/SDA/SDI"/>
<pin name="RC5/SDO"/>
<pin name="RC6/TX1/CCP3"/>
<pin name="RC7/RX1/CCP4"/>
<pin name="VSS@2"/>
<pin name="VDD"/>
<pin name="RB0/AN10/INT0"/>
<pin name="RB1/AN8/INT1"/>
<pin name="RB2/INT2/CANTX"/>
<pin name="RB3/INT3/CANRX"/>
<pin name="RB4/AN9"/>
<pin name="RB5/CCP5"/>
<pin name="RB6/TX2"/>
<pin name="RB7/RX2"/>
</symbol>
<symbol name="EM500">
<pin name="ACC"/>
<pin name="AVCC"/>
<pin name="TX+"/>
<pin name="TX-"/>
<pin name="RX+"/>
<pin name="RX-"/>
<pin name="SG"/>
<pin name="SR"/>
<pin name="SE"/>
<pin name="RST"/>
<pin name="MD"/>
<pin name="GND"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="P0.7"/>
<pin name="P0.6"/>
<pin name="P0.5"/>
<pin name="P0.4"/>
<pin name="P0.3"/>
<pin name="P0.2"/>
<pin name="P0.1/INT1"/>
<pin name="P0.0/INT0"/>
</symbol>
<symbol name="MCP1826">
<pin name="VOUT"/>
<pin name="GND@1"/>
<pin name="VIN"/>
<pin name="GND@2"/>
</symbol>
<symbol name="AT45DB041">
<pin name="SI"/>
<pin name="CLK"/>
<pin name="!RST"/>
<pin name="!CS"/>
<pin name="!WP"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="DS1340">
<pin name="X1"/>
<pin name="X2"/>
<pin name="VBAT"/>
<pin name="VSS"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="FT/OUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="MCP16301">
<description>High Voltage Input Integrated Switch Step-Down Regulator</description>
<pin name="BOOST"/>
<pin name="GND"/>
<pin name="VFB"/>
<pin name="EN"/>
<pin name="VIN"/>
<pin name="SW"/>
</symbol>
<symbol name="PESD2CAN">
<pin name="."/>
<pin name="..."/>
<pin name=".."/>
</symbol>
<symbol name="ADM3251E">
<pin name="NC"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="ROUT"/>
<pin name="TIN"/>
<pin name="GND@5"/>
<pin name="GNDISO"/>
<pin name="V-"/>
<pin name="C2-"/>
<pin name="C2+"/>
<pin name="RIN"/>
<pin name="TOUT"/>
<pin name="C1-"/>
<pin name="C1+"/>
<pin name="V+"/>
<pin name="VCCISO"/>
</symbol>
<symbol name="MCP1790">
<pin name="VOUT"/>
<pin name="GND@1"/>
<pin name="VIN"/>
<pin name="GND@2"/>
</symbol>
<symbol name="78MXX">
<pin name="VOUT"/>
<pin name="VIN"/>
<pin name="GND"/>
</symbol>
<symbol name="P6SMBXX">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CHOKE">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="HEADER-5">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="DIODE">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="TRANSISTOR-NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MCP2551">
<pin name="TXD"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="RXD"/>
<pin name="VREF"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="RS"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="ULN2003">
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="O1" direction="oc"/>
<pin name="O2" direction="oc"/>
<pin name="O3" direction="oc"/>
<pin name="O4" direction="oc"/>
<pin name="O5" direction="oc"/>
<pin name="O6" direction="oc"/>
<pin name="O7" direction="oc"/>
<pin name="CD+" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CAPACITOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAPACITOR-POLARIZED">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="HEADER-1">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="TERMINAL-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TERMINAL-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="DIL-24">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="RELAY_COILX2">
<pin name="-" direction="pas"/>
<pin name="R+" direction="pas"/>
<pin name="S+" direction="pas"/>
</symbol>
<symbol name="RELAY_SPDTX2">
<pin name="OA" direction="pas"/>
<pin name="SA" direction="pas"/>
<pin name="PA" direction="pas"/>
<pin name="SB" direction="pas"/>
<pin name="OB" direction="pas"/>
<pin name="PB" direction="pas"/>
</symbol>
<symbol name="RELAY_COIL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="RELAY_SPDT">
<pin name="NC" direction="pas"/>
<pin name="NO" direction="pas"/>
<pin name="COM" direction="pas"/>
</symbol>
<symbol name="RELAY_SPST">
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
</symbol>
<symbol name="RELAY_SPSTX2">
<pin name="SA" direction="pas"/>
<pin name="PA" direction="pas"/>
<pin name="SB" direction="pas"/>
<pin name="PB" direction="pas"/>
</symbol>
<symbol name="VARISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1PIN">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="DIODE-TRANSIL1">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="RJ45-SOCKET">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="RELAY_COILX2A">
<pin name="-" direction="pas"/>
<pin name="R+" direction="pas"/>
<pin name="S+" direction="pas"/>
</symbol>
<symbol name="HEADER-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RJ45-SOCKET+TRAFO">
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="5" direction="in"/>
<pin name="4" direction="in"/>
<pin name="C-R" direction="pas"/>
<pin name="A-R" direction="pas"/>
<pin name="C-L" direction="pas"/>
<pin name="A-L" direction="pas"/>
<pin name="M1" direction="pas"/>
<pin name="M2" direction="pas"/>
</symbol>
<symbol name="SUB-DF9">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
</symbol>
<symbol name="TRANSISTOR-MOSFET-N">
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="TLP250">
<pin name="NC@1"/>
<pin name="A"/>
<pin name="C"/>
<pin name="NC@2"/>
<pin name="GND"/>
<pin name="VO@1"/>
<pin name="VO@2"/>
<pin name="VCC"/>
</symbol>
<symbol name="DIODE-ZENER">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="DIODE-LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="DS18B20+">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="DQ"/>
</symbol>
<symbol name="MCP2561">
<pin name="TXD"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="RXD"/>
<pin name="SPLIT"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="STBY"/>
</symbol>
<symbol name="TOUCH_SENSOR">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="TRANSISTOR_IGBT_N">
<pin name="G" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="COUPLER-2CH-AC">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="E2"/>
<pin name="C2"/>
<pin name="E1"/>
<pin name="C1"/>
</symbol>
<symbol name="DIODE_BRIDGE">
<pin name="AC1" direction="pas"/>
<pin name="+" direction="pas"/>
<pin name="AC2" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="FUSE">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="ADUM1301">
<pin name="VDD1" direction="in"/>
<pin name="VDD2" direction="in"/>
<pin name="GND1@1" direction="in"/>
<pin name="GND2@1" direction="in"/>
<pin name="VIA" direction="in"/>
<pin name="VIB" direction="in"/>
<pin name="VIC" direction="in"/>
<pin name="GND1@2" direction="in"/>
<pin name="VOA" direction="hiz"/>
<pin name="VOB" direction="hiz"/>
<pin name="VOC" direction="hiz"/>
<pin name="VE2" direction="in"/>
<pin name="GND2@2" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="VE1" direction="in"/>
</symbol>
<symbol name="ADUM1401">
<pin name="VDD1" direction="in"/>
<pin name="VDD2" direction="in"/>
<pin name="GND1@1" direction="in"/>
<pin name="GND2@1" direction="in"/>
<pin name="VIA" direction="in"/>
<pin name="VIB" direction="in"/>
<pin name="VOC" direction="hiz"/>
<pin name="GND1@2" direction="in"/>
<pin name="VOA" direction="hiz"/>
<pin name="VOB" direction="hiz"/>
<pin name="VIC" direction="in"/>
<pin name="VE2" direction="in"/>
<pin name="GND2@2" direction="in"/>
<pin name="VOD" direction="hiz"/>
<pin name="VID" direction="in"/>
<pin name="VE1" direction="in"/>
</symbol>
<symbol name="COUPLER-1CH-AC">
<pin name="A1"/>
<pin name="A2"/>
<pin name="E1"/>
<pin name="C1"/>
</symbol>
<symbol name="IRS2127">
<pin name="VCC"/>
<pin name="IN"/>
<pin name="!FAULT"/>
<pin name="COM"/>
<pin name="VS"/>
<pin name="CS"/>
<pin name="HO"/>
<pin name="VB"/>
</symbol>
<symbol name="6N135">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
</symbol>
<symbol name="IRS2128">
<pin name="VCC"/>
<pin name="!IN"/>
<pin name="!FAULT"/>
<pin name="COM"/>
<pin name="VS"/>
<pin name="CS"/>
<pin name="HO"/>
<pin name="VB"/>
</symbol>
<symbol name="COUPLER-1CH">
<pin name="A"/>
<pin name="K"/>
<pin name="E"/>
<pin name="C"/>
</symbol>
<symbol name="THYRISTOR">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="THERMISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="HEATSINK">
<description>HAPCAN Heatsink</description>
</symbol>
<symbol name="MCP9509">
<description>Resistor-Programmable Temperature Switch</description>
<pin name="SET"/>
<pin name="GND"/>
<pin name="!OUT"/>
<pin name="HYST"/>
<pin name="VDD"/>
</symbol>
<symbol name="MCP23017">
<description>16-Bit I/O Expander with Serial Interface</description>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="INTA" direction="out"/>
<pin name="INTB" direction="out"/>
<pin name="GPB0"/>
<pin name="GPB1"/>
<pin name="GPB2"/>
<pin name="GPB3"/>
<pin name="GPB4"/>
<pin name="GPB5"/>
<pin name="GPB6"/>
<pin name="GPB7"/>
<pin name="GPA0"/>
<pin name="GPA1"/>
<pin name="GPA2"/>
<pin name="GPA3"/>
<pin name="GPA4"/>
<pin name="GPA5"/>
<pin name="GPA6"/>
<pin name="GPA7"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="ADUM1251">
<description>Hot Swappable, Dual I2C Isolator</description>
<pin name="VDD1" direction="pwr"/>
<pin name="SDA1"/>
<pin name="SCL1" direction="in"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="SCL2" direction="out"/>
<pin name="SDA2"/>
<pin name="VDD2" direction="pwr"/>
</symbol>
<symbol name="TERMINAL-1">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="UNIV3CPU" prefix="IC" uservalue="yes">
<description>HAPCAN Microcontroller UNIV 3 CPU</description>
<gates>
<gate name="G$1" symbol="UNIV3CPU"/>
</gates>
<devices>
<device name="-I/SO" package="UNIV3CPU">
<connects>
<connect gate="G$1" pin="!MCLR!/RE3" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKIN/RA7" pad="9"/>
<connect gate="G$1" pin="OSC2/CLKOUT/RA6" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/AN10/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/AN8/INT1" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/CANTX" pad="23"/>
<connect gate="G$1" pin="RB3/INT3/CANRX" pad="24"/>
<connect gate="G$1" pin="RB4/AN9" pad="25"/>
<connect gate="G$1" pin="RB5/CCP5" pad="26"/>
<connect gate="G$1" pin="RB6/TX2" pad="27"/>
<connect gate="G$1" pin="RB7/RX2" pad="28"/>
<connect gate="G$1" pin="RC0/SCLKI" pad="11"/>
<connect gate="G$1" pin="RC1/ISOSCI" pad="12"/>
<connect gate="G$1" pin="RC2/CCP2" pad="13"/>
<connect gate="G$1" pin="RC3/SCL/SCK" pad="14"/>
<connect gate="G$1" pin="RC4/SDA/SDI" pad="15"/>
<connect gate="G$1" pin="RC5/SDO" pad="16"/>
<connect gate="G$1" pin="RC6/TX1/CCP3" pad="17"/>
<connect gate="G$1" pin="RC7/RX1/CCP4" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDCORE" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM500">
<description>Tibbo programmable ethernet module</description>
<gates>
<gate name="G$1" symbol="EM500"/>
</gates>
<devices>
<device name="EM500" package="EM500">
<connects>
<connect gate="G$1" pin="ACC" pad="22"/>
<connect gate="G$1" pin="AVCC" pad="21"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="MD" pad="12"/>
<connect gate="G$1" pin="P0.0/INT0" pad="1"/>
<connect gate="G$1" pin="P0.1/INT1" pad="2"/>
<connect gate="G$1" pin="P0.2" pad="3"/>
<connect gate="G$1" pin="P0.3" pad="4"/>
<connect gate="G$1" pin="P0.4" pad="5"/>
<connect gate="G$1" pin="P0.5" pad="6"/>
<connect gate="G$1" pin="P0.6" pad="7"/>
<connect gate="G$1" pin="P0.7" pad="8"/>
<connect gate="G$1" pin="RST" pad="13"/>
<connect gate="G$1" pin="RX" pad="9"/>
<connect gate="G$1" pin="RX+" pad="18"/>
<connect gate="G$1" pin="RX-" pad="17"/>
<connect gate="G$1" pin="SE" pad="14"/>
<connect gate="G$1" pin="SG" pad="16"/>
<connect gate="G$1" pin="SR" pad="15"/>
<connect gate="G$1" pin="TX" pad="10"/>
<connect gate="G$1" pin="TX+" pad="20"/>
<connect gate="G$1" pin="TX-" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1826" prefix="IC">
<description>1000 mA, Low Voltage, Low Quiescent Current
LDO Regulator</description>
<gates>
<gate name="G$1" symbol="MCP1826"/>
</gates>
<devices>
<device name="SOT223-3" package="SOT-223">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB041" prefix="IC">
<gates>
<gate name="G$1" symbol="AT45DB041"/>
</gates>
<devices>
<device name="SO8" package="SO-08">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="!WP" pad="5"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1340Z" prefix="IC">
<description>DS1340Z</description>
<gates>
<gate name="G$1" symbol="DS1340"/>
</gates>
<devices>
<device name="SO-08" package="SO-08">
<connects>
<connect gate="G$1" pin="FT/OUT" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP16301" prefix="IC">
<description>High Voltage Input Integrated Switch Step-Down Regulator</description>
<gates>
<gate name="G$1" symbol="MCP16301"/>
</gates>
<devices>
<device name="SOT23-6" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="BOOST" pad="1"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="6"/>
<connect gate="G$1" pin="VFB" pad="3"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD2CAN" prefix="D">
<description>CAN bus ESD protection diode</description>
<gates>
<gate name="G$1" symbol="PESD2CAN"/>
</gates>
<devices>
<device name="SOT-23" package="SOT-23">
<connects>
<connect gate="G$1" pin="." pad="1"/>
<connect gate="G$1" pin=".." pad="2"/>
<connect gate="G$1" pin="..." pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADM3251E" prefix="IC" uservalue="yes">
<description>RS232C isolated transceiver</description>
<gates>
<gate name="G$1" symbol="ADM3251E"/>
</gates>
<devices>
<device name="" package="SO-20W">
<connects>
<connect gate="G$1" pin="C1+" pad="18"/>
<connect gate="G$1" pin="C1-" pad="17"/>
<connect gate="G$1" pin="C2+" pad="14"/>
<connect gate="G$1" pin="C2-" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="7"/>
<connect gate="G$1" pin="GND@5" pad="10"/>
<connect gate="G$1" pin="GNDISO" pad="11"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RIN" pad="15"/>
<connect gate="G$1" pin="ROUT" pad="8"/>
<connect gate="G$1" pin="TIN" pad="9"/>
<connect gate="G$1" pin="TOUT" pad="16"/>
<connect gate="G$1" pin="V+" pad="19"/>
<connect gate="G$1" pin="V-" pad="12"/>
<connect gate="G$1" pin="VCC@1" pad="2"/>
<connect gate="G$1" pin="VCC@2" pad="3"/>
<connect gate="G$1" pin="VCCISO" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1790" prefix="IC">
<description>70 mA, High Voltage Regulator</description>
<gates>
<gate name="G$1" symbol="MCP1790"/>
</gates>
<devices>
<device name="" package="SOT-223">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78XX" prefix="IC">
<description>HAPCAN positive voltage regulator</description>
<gates>
<gate name="G$1" symbol="78MXX"/>
</gates>
<devices>
<device name="_TO-252" package="TO-252">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO-92" package="TO-92">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO-220V" package="TO220V">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SOT-23" package="SOT-23">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_TRANSIL2" prefix="D">
<description>HAPCAN Bidirectional transil diode</description>
<gates>
<gate name="1" symbol="P6SMBXX"/>
</gates>
<devices>
<device name="" package="DO-214_TRANSIL2">
<connects>
<connect gate="1" pin="1" pad="A"/>
<connect gate="1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHOKE" prefix="L" uservalue="yes">
<description>Choke</description>
<gates>
<gate name="G$1" symbol="CHOKE"/>
</gates>
<devices>
<device name="DL16" package="CHOKE-DL16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10X25" package="CHOKE-10X25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DER0705" package="CHOKE-DER0705">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER5" prefix="JP">
<description>HAPCAN Header 5</description>
<gates>
<gate name="G$1" symbol="HEADER-5"/>
</gates>
<devices>
<device name="" package="SIP-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="SIP-5A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D">
<description>HAPCAN Rectifier Diode</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="_DO-214" package="DO-214">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="0805">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO220V" package="TO220V-2">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MELF" package="DO-213">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MINIMELF" package="SOD-80">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_NPN" prefix="Q" uservalue="yes">
<description>HAPCAN NPN Transistor</description>
<gates>
<gate name="G$1" symbol="TRANSISTOR-NPN"/>
</gates>
<devices>
<device name="" package="SOT-23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP2551" prefix="IC">
<description>HAPCAN CAN Tranceiver</description>
<gates>
<gate name="G$1" symbol="MCP2551"/>
</gates>
<devices>
<device name="-I/SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Y">
<description>HAPCAN Crystal</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="-HC49V" package="CRYSTAL-HC49V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TC26V" package="CRYSTAL-TC26V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TC38H" package="CRYSTAL-TC38H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULN2003" prefix="IC">
<description>HAPCAN 7 channel Darlington Array NPN 50V 0.5A</description>
<gates>
<gate name="A" symbol="ULN2003"/>
</gates>
<devices>
<device name="" package="SO-16">
<connects>
<connect gate="A" pin="CD+" pad="9"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="I1" pad="1"/>
<connect gate="A" pin="I2" pad="2"/>
<connect gate="A" pin="I3" pad="3"/>
<connect gate="A" pin="I4" pad="4"/>
<connect gate="A" pin="I5" pad="5"/>
<connect gate="A" pin="I6" pad="6"/>
<connect gate="A" pin="I7" pad="7"/>
<connect gate="A" pin="O1" pad="16"/>
<connect gate="A" pin="O2" pad="15"/>
<connect gate="A" pin="O3" pad="14"/>
<connect gate="A" pin="O4" pad="13"/>
<connect gate="A" pin="O5" pad="12"/>
<connect gate="A" pin="O6" pad="11"/>
<connect gate="A" pin="O7" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR" prefix="C">
<description>HAPCAN Capacitor</description>
<gates>
<gate name="G$1" symbol="CAPACITOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="15X5" package="CAP-15X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10X6" package="CAP-10X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR-POLARIZED" prefix="C">
<description>HAPCAN Polarazied Capacitor</description>
<gates>
<gate name="G$1" symbol="CAPACITOR-POLARIZED"/>
</gates>
<devices>
<device name="-SMC_C" package="SMC_C">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMC_B" package="SMC_B">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMC_D" package="SMC_D">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5X10.5" package="CAP-5X10.5">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5X14" package="CAP-5X14">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2X5" package="CAP-2X5">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R">
<description>HAPCAN Resistor</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="15X5" package="RES-15X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.8X3V" package="RES-3.8X3V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER1" prefix="JP">
<description>HAPCAN Header 1</description>
<gates>
<gate name="G$1" symbol="HEADER-1"/>
</gates>
<devices>
<device name="1X0.9" package="SIP-1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X1.3" package="HEADER-1X1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERMINAL-2" prefix="CON">
<description>HAPCAN Terminal Block - 2 way</description>
<gates>
<gate name="G$1" symbol="TERMINAL-2"/>
</gates>
<devices>
<device name="-5X9MM" package="ARK2-5X9MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5X10,5MM" package="ARK2-5X10,5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7.5X10.5MM" package="ARK2-7.5X10.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERMINAL-3" prefix="CON">
<description>HAPCAN Terminal Block - 3 way</description>
<gates>
<gate name="G$1" symbol="TERMINAL-3"/>
</gates>
<devices>
<device name="-5X9MM" package="ARK3-5X9MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5X10.5MM" package="ARK3-5X10.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7.5X10.5MM" package="ARK3-7.5X10.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIL-24" prefix="JP">
<description>HAPCAN DIL-24</description>
<gates>
<gate name="G$1" symbol="DIL-24"/>
</gates>
<devices>
<device name="" package="DIL-24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY_RT" prefix="K">
<description>HAPCAN Bistable relay 16A</description>
<gates>
<gate name="2" symbol="RELAY_SPDTX2"/>
<gate name="G$1" symbol="RELAY_COILX2A"/>
</gates>
<devices>
<device name="" package="RELAY_RT">
<connects>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
<connect gate="G$1" pin="-" pad="A3"/>
<connect gate="G$1" pin="R+" pad="A2"/>
<connect gate="G$1" pin="S+" pad="A1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY_PE" prefix="K">
<description>HAPCAN Monostable relay 5A</description>
<gates>
<gate name="1" symbol="RELAY_COIL"/>
<gate name="2" symbol="RELAY_SPDT"/>
</gates>
<devices>
<device name="" package="RELAY_PE">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="COM" pad="11"/>
<connect gate="2" pin="NC" pad="12"/>
<connect gate="2" pin="NO" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY_PE+RT" prefix="K">
<description>HAPCAN Mono/Bistable relay 5A/16A together</description>
<gates>
<gate name="G$1" symbol="RELAY_COIL"/>
<gate name="G$2" symbol="RELAY_COILX2"/>
<gate name="G$3" symbol="RELAY_SPST"/>
<gate name="G$4" symbol="RELAY_SPSTX2"/>
</gates>
<devices>
<device name="" package="RELAY_PE+RT">
<connects>
<connect gate="G$1" pin="1" pad="A4"/>
<connect gate="G$1" pin="2" pad="A5"/>
<connect gate="G$2" pin="-" pad="A3"/>
<connect gate="G$2" pin="R+" pad="A2"/>
<connect gate="G$2" pin="S+" pad="A1"/>
<connect gate="G$3" pin="P" pad="11"/>
<connect gate="G$3" pin="S" pad="14"/>
<connect gate="G$4" pin="PA" pad="11A"/>
<connect gate="G$4" pin="PB" pad="11B"/>
<connect gate="G$4" pin="SA" pad="14A"/>
<connect gate="G$4" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VARISTOR" prefix="R">
<description>HAPCAN Varistor</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="7.5MM-1" package="VARISTOR1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.0MM-1" package="VARISTOR2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7.5MM-2" package="VARISTOR3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM-1" package="VARISTOR4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2X8" prefix="CON" uservalue="yes">
<description>16pin connector 2.54 raster</description>
<gates>
<gate name="1" symbol="CONNECTOR-1PIN"/>
<gate name="2" symbol="CONNECTOR-1PIN"/>
<gate name="3" symbol="CONNECTOR-1PIN"/>
<gate name="4" symbol="CONNECTOR-1PIN"/>
<gate name="5" symbol="CONNECTOR-1PIN"/>
<gate name="6" symbol="CONNECTOR-1PIN"/>
<gate name="7" symbol="CONNECTOR-1PIN"/>
<gate name="8" symbol="CONNECTOR-1PIN"/>
<gate name="9" symbol="CONNECTOR-1PIN"/>
<gate name="10" symbol="CONNECTOR-1PIN"/>
<gate name="11" symbol="CONNECTOR-1PIN"/>
<gate name="12" symbol="CONNECTOR-1PIN"/>
<gate name="13" symbol="CONNECTOR-1PIN"/>
<gate name="14" symbol="CONNECTOR-1PIN"/>
<gate name="15" symbol="CONNECTOR-1PIN"/>
<gate name="16" symbol="CONNECTOR-1PIN"/>
</gates>
<devices>
<device name="_NORMAL" package="HEADER-2X8">
<connects>
<connect gate="1" pin="S" pad="1"/>
<connect gate="10" pin="S" pad="10"/>
<connect gate="11" pin="S" pad="11"/>
<connect gate="12" pin="S" pad="12"/>
<connect gate="13" pin="S" pad="13"/>
<connect gate="14" pin="S" pad="14"/>
<connect gate="15" pin="S" pad="15"/>
<connect gate="16" pin="S" pad="16"/>
<connect gate="2" pin="S" pad="2"/>
<connect gate="3" pin="S" pad="3"/>
<connect gate="4" pin="S" pad="4"/>
<connect gate="5" pin="S" pad="5"/>
<connect gate="6" pin="S" pad="6"/>
<connect gate="7" pin="S" pad="7"/>
<connect gate="8" pin="S" pad="8"/>
<connect gate="9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MIRRORED" package="HEADER-2X8-MIRRORED">
<connects>
<connect gate="1" pin="S" pad="1"/>
<connect gate="10" pin="S" pad="10"/>
<connect gate="11" pin="S" pad="11"/>
<connect gate="12" pin="S" pad="12"/>
<connect gate="13" pin="S" pad="13"/>
<connect gate="14" pin="S" pad="14"/>
<connect gate="15" pin="S" pad="15"/>
<connect gate="16" pin="S" pad="16"/>
<connect gate="2" pin="S" pad="2"/>
<connect gate="3" pin="S" pad="3"/>
<connect gate="4" pin="S" pad="4"/>
<connect gate="5" pin="S" pad="5"/>
<connect gate="6" pin="S" pad="6"/>
<connect gate="7" pin="S" pad="7"/>
<connect gate="8" pin="S" pad="8"/>
<connect gate="9" pin="S" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SMD" package="HEADER-2X8_SMD">
<connects>
<connect gate="1" pin="S" pad="P$1"/>
<connect gate="10" pin="S" pad="P$10"/>
<connect gate="11" pin="S" pad="P$11"/>
<connect gate="12" pin="S" pad="P$12"/>
<connect gate="13" pin="S" pad="P$13"/>
<connect gate="14" pin="S" pad="P$14"/>
<connect gate="15" pin="S" pad="P$15"/>
<connect gate="16" pin="S" pad="P$16"/>
<connect gate="2" pin="S" pad="P$2"/>
<connect gate="3" pin="S" pad="P$3"/>
<connect gate="4" pin="S" pad="P$4"/>
<connect gate="5" pin="S" pad="P$5"/>
<connect gate="6" pin="S" pad="P$6"/>
<connect gate="7" pin="S" pad="P$7"/>
<connect gate="8" pin="S" pad="P$8"/>
<connect gate="9" pin="S" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_TRANSIL1" prefix="D" uservalue="yes">
<description>HAPCAN Unidirectional transil diode</description>
<gates>
<gate name="G$1" symbol="DIODE-TRANSIL1"/>
</gates>
<devices>
<device name="_DO214" package="DO-214">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MINIMELF" package="SOD-80">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45-SOCKET" prefix="CON">
<description>HAPCAN RJ45 socket</description>
<gates>
<gate name="G$1" symbol="RJ45-SOCKET"/>
</gates>
<devices>
<device name="" package="RJ45-PCB-SOCKET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2" prefix="JP">
<description>HAPCAN Header 2</description>
<gates>
<gate name="G$1" symbol="HEADER-2"/>
</gates>
<devices>
<device name="" package="SIP-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45-SOCKET-LMJ2018811100DL1T4" prefix="CON">
<description>AMPHENOL LMJ2018811100DL1T4</description>
<gates>
<gate name="G$1" symbol="RJ45-SOCKET+TRAFO"/>
</gates>
<devices>
<device name="" package="RJ45-PCB-SOCKET+TRAFO">
<connects>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A-L" pad="10"/>
<connect gate="G$1" pin="A-R" pad="12"/>
<connect gate="G$1" pin="C-L" pad="9"/>
<connect gate="G$1" pin="C-R" pad="11"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUB-DF9" prefix="CON">
<description>HAPCAN SUB-D 9 pin female connector</description>
<gates>
<gate name="G$1" symbol="SUB-DF9"/>
</gates>
<devices>
<device name="" package="SUB-D9FH-7.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="G1" pad="M1"/>
<connect gate="G$1" pin="G2" pad="M2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_MOSFET_N" prefix="Q">
<description>HAPCAN N-MOSFET</description>
<gates>
<gate name="G$1" symbol="TRANSISTOR-MOSFET-N"/>
</gates>
<devices>
<device name="_TO220V" package="TO220V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO247V" package="TO247V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO220V-3" package="TO220V-3">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLP250" prefix="IC">
<description>TLP250</description>
<gates>
<gate name="G$1" symbol="TLP250"/>
</gates>
<devices>
<device name="" package="DIL-08">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@2" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VO@1" pad="6"/>
<connect gate="G$1" pin="VO@2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_WIDE" package="DIL-08W">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@2" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VO@1" pad="6"/>
<connect gate="G$1" pin="VO@2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_ZENER" prefix="D">
<description>HAPCAN ZENER DIODE</description>
<gates>
<gate name="G$1" symbol="DIODE-ZENER"/>
</gates>
<devices>
<device name="_SOD-80" package="SOD-80">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_DO-214" package="DO-214">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_LED" prefix="D" uservalue="yes">
<description>HAPCAN LED diode</description>
<gates>
<gate name="G$1" symbol="DIODE-LED"/>
</gates>
<devices>
<device name="_1206" package="1206_LED-R">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS18B20+" prefix="IC">
<description>HAPCAN DS18B20+ temperature sensor</description>
<gates>
<gate name="G$1" symbol="DS18B20+"/>
</gates>
<devices>
<device name="_TO-92" package="TO-92">
<connects>
<connect gate="G$1" pin="DQ" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO-92_SMD" package="TO-92_SMD">
<connects>
<connect gate="G$1" pin="DQ" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP2561" prefix="IC">
<description>HAPCAN CAN Tranceiver</description>
<gates>
<gate name="G$1" symbol="MCP2561"/>
</gates>
<devices>
<device name="-E/SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SPLIT" pad="5"/>
<connect gate="G$1" pin="STBY" pad="8"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH_SENSOR" prefix="S">
<description>HAPCAN touch sensor</description>
<gates>
<gate name="G$1" symbol="TOUCH_SENSOR"/>
</gates>
<devices>
<device name="" package="TOUCH_SENSOR">
<connects>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_IGBT_N" prefix="Q">
<description>HAPCAN IGBT transistor</description>
<gates>
<gate name="G$1" symbol="TRANSISTOR_IGBT_N"/>
</gates>
<devices>
<device name="_TO247H" package="TO247H">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO247V" package="TO247V">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO220H" package="TO220H">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO220V" package="TO220V">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COUPLER-2CH-AC" prefix="IC">
<description>COUPLER-2CH-AC</description>
<gates>
<gate name="G$1" symbol="COUPLER-2CH-AC"/>
</gates>
<devices>
<device name="_WIDE" package="DIL-08W">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="A4" pad="4"/>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="C2" pad="6"/>
<connect gate="G$1" pin="E1" pad="7"/>
<connect gate="G$1" pin="E2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_BRIDGE" prefix="B">
<description>HAPCAN Single Phase Bridge Rectifier</description>
<gates>
<gate name="G$1" symbol="DIODE_BRIDGE"/>
</gates>
<devices>
<device name="-3.8" package="RECTIFIER_KBL">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="AC1" pad="AC1"/>
<connect gate="G$1" pin="AC2" pad="AC2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5.0" package="RECTIFIER_KBP">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="AC1" pad="AC1"/>
<connect gate="G$1" pin="AC2" pad="AC2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="RECTIFIER_DBS">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="AC1" pad="AC1"/>
<connect gate="G$1" pin="AC2" pad="AC2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TO-269" package="TO-269AA">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="AC1" pad="AC1"/>
<connect gate="G$1" pin="AC2" pad="AC2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FUSE" prefix="F" uservalue="yes">
<description>HAPCAN fuse</description>
<gates>
<gate name="G$1" symbol="FUSE"/>
</gates>
<devices>
<device name="_V" package="FUSE-HOLDER-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TERM" package="FUSE-LITTLEFUSE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_UMT" package="FUSE-UMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="FUSE-7.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUM1301" prefix="IC">
<description>Triple-Channel Digital Isolators</description>
<gates>
<gate name="G$1" symbol="ADUM1301"/>
</gates>
<devices>
<device name="" package="SO-16W">
<connects>
<connect gate="G$1" pin="GND1@1" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="8"/>
<connect gate="G$1" pin="GND2@1" pad="15"/>
<connect gate="G$1" pin="GND2@2" pad="9"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="11"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VE1" pad="7"/>
<connect gate="G$1" pin="VE2" pad="10"/>
<connect gate="G$1" pin="VIA" pad="3"/>
<connect gate="G$1" pin="VIB" pad="4"/>
<connect gate="G$1" pin="VIC" pad="12"/>
<connect gate="G$1" pin="VOA" pad="14"/>
<connect gate="G$1" pin="VOB" pad="13"/>
<connect gate="G$1" pin="VOC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUM1401" prefix="IC">
<description>Quadruple-Channel Digital Isolators</description>
<gates>
<gate name="G$1" symbol="ADUM1401"/>
</gates>
<devices>
<device name="" package="SO-16W">
<connects>
<connect gate="G$1" pin="GND1@1" pad="3"/>
<connect gate="G$1" pin="GND1@2" pad="9"/>
<connect gate="G$1" pin="GND2@1" pad="16"/>
<connect gate="G$1" pin="GND2@2" pad="10"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="1"/>
<connect gate="G$1" pin="VE1" pad="8"/>
<connect gate="G$1" pin="VE2" pad="11"/>
<connect gate="G$1" pin="VIA" pad="4"/>
<connect gate="G$1" pin="VIB" pad="5"/>
<connect gate="G$1" pin="VIC" pad="6"/>
<connect gate="G$1" pin="VID" pad="12"/>
<connect gate="G$1" pin="VOA" pad="15"/>
<connect gate="G$1" pin="VOB" pad="14"/>
<connect gate="G$1" pin="VOC" pad="13"/>
<connect gate="G$1" pin="VOD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COUPLER-1CH-AC" prefix="IC" uservalue="yes">
<description>COUPLER-1CH-AC</description>
<gates>
<gate name="G$1" symbol="COUPLER-1CH-AC"/>
</gates>
<devices>
<device name="_SMD" package="SMD4">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C1" pad="4"/>
<connect gate="G$1" pin="E1" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_WIDE" package="DIL-04W">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C1" pad="4"/>
<connect gate="G$1" pin="E1" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2127" prefix="IC" uservalue="yes">
<description>IGBT driver with current sensing and undervoltage lockout</description>
<gates>
<gate name="G$1" symbol="IRS2127"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="!FAULT" pad="3"/>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="HO" pad="7"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="VB" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6N135" prefix="IC" uservalue="yes">
<description>6N136 optocoupler</description>
<gates>
<gate name="A" symbol="6N135"/>
</gates>
<devices>
<device name="" package="DIL-08W">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2128" prefix="IC" uservalue="yes">
<description>IGBT driver with current sensing and undervoltage lockout (negative input)</description>
<gates>
<gate name="G$1" symbol="IRS2128"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="!FAULT" pad="3"/>
<connect gate="G$1" pin="!IN" pad="2"/>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="HO" pad="7"/>
<connect gate="G$1" pin="VB" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2X4" prefix="CON" uservalue="yes">
<description>8pin connector 2.54 raster</description>
<gates>
<gate name="1" symbol="CONNECTOR-1PIN"/>
<gate name="2" symbol="CONNECTOR-1PIN"/>
<gate name="3" symbol="CONNECTOR-1PIN"/>
<gate name="4" symbol="CONNECTOR-1PIN"/>
<gate name="5" symbol="CONNECTOR-1PIN"/>
<gate name="6" symbol="CONNECTOR-1PIN"/>
<gate name="7" symbol="CONNECTOR-1PIN"/>
<gate name="8" symbol="CONNECTOR-1PIN"/>
</gates>
<devices>
<device name="_NORMAL" package="HEADER-2X4">
<connects>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="S" pad="2"/>
<connect gate="3" pin="S" pad="3"/>
<connect gate="4" pin="S" pad="4"/>
<connect gate="5" pin="S" pad="5"/>
<connect gate="6" pin="S" pad="6"/>
<connect gate="7" pin="S" pad="7"/>
<connect gate="8" pin="S" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MIRRORED" package="HEADER-2X4-MIRRORED">
<connects>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="S" pad="2"/>
<connect gate="3" pin="S" pad="3"/>
<connect gate="4" pin="S" pad="4"/>
<connect gate="5" pin="S" pad="5"/>
<connect gate="6" pin="S" pad="6"/>
<connect gate="7" pin="S" pad="7"/>
<connect gate="8" pin="S" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY_RT_SPST" prefix="K">
<description>HAPCAN Bistable relay 16A - SPST (single pole, single throw)</description>
<gates>
<gate name="G$2" symbol="RELAY_SPSTX2"/>
<gate name="G$1" symbol="RELAY_COILX2A"/>
</gates>
<devices>
<device name="" package="RELAY_RT_SPST">
<connects>
<connect gate="G$1" pin="-" pad="A3"/>
<connect gate="G$1" pin="R+" pad="A2"/>
<connect gate="G$1" pin="S+" pad="A1"/>
<connect gate="G$2" pin="PA" pad="11A"/>
<connect gate="G$2" pin="PB" pad="11B"/>
<connect gate="G$2" pin="SA" pad="14A"/>
<connect gate="G$2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY_SNR_SPDT" prefix="K">
<description>HAPCAN Slim PCB Relay 6 A - SPDT (single pole, double throw)</description>
<gates>
<gate name="G$1" symbol="RELAY_COIL"/>
<gate name="G$2" symbol="RELAY_SPDT"/>
</gates>
<devices>
<device name="V" package="RELAY_SNR_SPDT_V">
<connects>
<connect gate="G$1" pin="1" pad="A1"/>
<connect gate="G$1" pin="2" pad="A2"/>
<connect gate="G$2" pin="COM" pad="11"/>
<connect gate="G$2" pin="NC" pad="12"/>
<connect gate="G$2" pin="NO" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="RELAY_SNR_SPDT_H">
<connects>
<connect gate="G$1" pin="1" pad="A1"/>
<connect gate="G$1" pin="2" pad="A2"/>
<connect gate="G$2" pin="COM" pad="11"/>
<connect gate="G$2" pin="NC" pad="12"/>
<connect gate="G$2" pin="NO" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COUPLER-1CH" prefix="IC">
<description>COUPLER-1CH</description>
<gates>
<gate name="G$1" symbol="COUPLER-1CH"/>
</gates>
<devices>
<device name="_04W" package="DIL-04W">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="THYRISTOR" prefix="Q">
<description>HAPCAN Thyristor</description>
<gates>
<gate name="G$1" symbol="THYRISTOR"/>
</gates>
<devices>
<device name="_SOT23" package="SOT-23">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="G" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SOT223" package="SOT-223">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1 4"/>
<connect gate="G$1" pin="G" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="THERMISTOR" prefix="R">
<description>HAPCAN Thermistor</description>
<gates>
<gate name="G$1" symbol="THERMISTOR"/>
</gates>
<devices>
<device name="_0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEATSINK">
<description>HAPCAN Heatsink</description>
<gates>
<gate name="G$1" symbol="HEATSINK"/>
</gates>
<devices>
<device name="_HS003" package="HEATSINK_HS-003">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HS123" package="HEATSINK_HS-123">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP9509" prefix="IC">
<description>Resistor-Programmable Temperature Switch</description>
<gates>
<gate name="G$1" symbol="MCP9509"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="!OUT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="HYST" pad="4"/>
<connect gate="G$1" pin="SET" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23017" prefix="IC" uservalue="yes">
<description>16-Bit I/O Expander with Serial Interface</description>
<gates>
<gate name="G$1" symbol="MCP23017"/>
</gates>
<devices>
<device name="-SO" package="SO-28W">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUM1251" prefix="IC">
<description>Hot Swappable, Dual I2C Isolator</description>
<gates>
<gate name="G$1" symbol="ADUM1251"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="SCL1" pad="3"/>
<connect gate="G$1" pin="SCL2" pad="6"/>
<connect gate="G$1" pin="SDA1" pad="2"/>
<connect gate="G$1" pin="SDA2" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MKKDS1/8-3,5" prefix="CON">
<description>Terminal block MKKDS 1/8-3,5</description>
<gates>
<gate name="-1" symbol="TERMINAL-1"/>
<gate name="-2" symbol="TERMINAL-1"/>
<gate name="-3" symbol="TERMINAL-1"/>
<gate name="-4" symbol="TERMINAL-1"/>
<gate name="-5" symbol="TERMINAL-1"/>
<gate name="-6" symbol="TERMINAL-1"/>
<gate name="-7" symbol="TERMINAL-1"/>
<gate name="-8" symbol="TERMINAL-1"/>
<gate name="-9" symbol="TERMINAL-1"/>
<gate name="-10" symbol="TERMINAL-1"/>
<gate name="-11" symbol="TERMINAL-1"/>
<gate name="-12" symbol="TERMINAL-1"/>
<gate name="-13" symbol="TERMINAL-1"/>
<gate name="-14" symbol="TERMINAL-1"/>
<gate name="-15" symbol="TERMINAL-1"/>
<gate name="-16" symbol="TERMINAL-1"/>
</gates>
<devices>
<device name="" package="MKKDS1/8-3,5">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-10" pin="1" pad="10"/>
<connect gate="-11" pin="1" pad="11"/>
<connect gate="-12" pin="1" pad="12"/>
<connect gate="-13" pin="1" pad="13"/>
<connect gate="-14" pin="1" pad="14"/>
<connect gate="-15" pin="1" pad="15"/>
<connect gate="-16" pin="1" pad="16"/>
<connect gate="-2" pin="1" pad="2"/>
<connect gate="-3" pin="1" pad="3"/>
<connect gate="-4" pin="1" pad="4"/>
<connect gate="-5" pin="1" pad="5"/>
<connect gate="-6" pin="1" pad="6"/>
<connect gate="-7" pin="1" pad="7"/>
<connect gate="-8" pin="1" pad="8"/>
<connect gate="-9" pin="1" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
